Change Log V1.2.2a 18Nov09

1) Fixed Internet Radio Shoutcast IP change
2) Added "search function" Internet Radio
3) Fixed DVD subtitle problem
4) Fixed some spelling mistakes
5) Fixed Hard Drive size reading error on setup Info screen
6) Fixed video info information (video and audio were swopped)
7) Fixed File Copy Network Login screen

Firmware Update Instructions
Copy install.img and logo_pal_bmp to the root directory of a Flash Drive. Plug the flash drive into the Mede8er. 

1) Go to the Setup menu and then select System and then select System Update. 
2) Select Save Config
3) Select System Update again 
4) The Mede8er will now start the Firmware Update procedure. During update your TV screen will go blank and 
   the Mede8er will re boot and then display update bars on the TV. Mede8er will inform you when the update 
   procedure is completed.

XXXX  IF YOU DO NOT GET A PICTURE ON YOUR TV DURING THE UPDATE PROCEDURE JUST CHECK THAT THE LED ON 
         THE MEDE8ER IS FLASHING RED-BLUE AND WAIT UNTILL THE LED STOPS FLASHING AND THE MEDE8ER RE BOOTS  XXXXX

5) Once completed the Mede8er will re boot.
6) Go to the Setup menu and then select System and then select System Update.
7) Select Restore Config
8) The Mede8er will re boot and the firmware update procedure is complete. 

DURING UPDATE THE LED ON THE MEDE8ER WILL FLASH BLUE/RED. PLEASE WAIT UNTIL THE MEDE8ER RE BOOTS.  

xxxxxxxxxxxx DO NOT REMOVE POWER DURING THE UPDATE PROCESS xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx   

Emergency Recovery Procedure

Download the latest Firmware from the Mede8er website. Unzip the file and you will find two files ie install.img  
and logo_pal_bmp. Copy both these files to the root directory of a Flash Drive. Plug the flash drive into the Mede8er. 
Power the Mede8er down. Power up again and hold the on/off button for 10 seconds and the unit will automatically 
re install the Firmware.          

xxxxxxxxxxxx DO NOT REMOVE POWER DURING THE UPDATE PROCESS xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx 

128M-HMC-M03I-20091118-v7.0.7.r2089_SANJIA_USB
