Change Log V2.1.0 4March2010

1) Fixed NTFS driver problems
2) Fixed HDD Formatt issue
3) Fixed streaming/USB issues when no HDD installed in Mede8er 

Known Bugs
1) Front LED does not light on standby
2) Screen Size adjust numerical display in Setup Menu always shows 1280 x 720 pixel size
    


Use Emergency Firmware Procedure (Do not use update via GUI)

Download the latest Firmware from the Mede8er website. Unzip the file and you will find two files ie install.img  
and logo_pal_bmp. Copy both these files to the root directory of a Flash Drive. Plug the flash drive into the Mede8er. 
Power the Mede8er down. Power up again and hold the on/off button for 10 seconds then release.          

The Mede8er will now start the Firmware Update procedure. During update your TV screen will go blank and 
the Mede8er will re boot and then display update bars on the TV. Mede8er will inform you when the update 
procedure is completed.

XXXX  IF YOU DO NOT GET A PICTURE ON YOUR TV DURING THE UPDATE PROCEDURE JUST CHECK THAT THE LED ON 
      THE MEDE8ER IS FLASHING RED-BLUE AND WAIT UNTILL THE LED STOPS FLASHING AND THE MEDE8ER RE BOOTS  XXXXX

xxxxxxxxxxxx DO NOT REMOVE POWER DURING THE UPDATE PROCESS xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx 


